# Release Notes for STM32F0xx Standard Peripherals Library Examples Copyright 2014 STMicroelectronics
## Update History ### V1.4.0 / 24-July-2014 Main Changes Update PWR_Standby and PWR_CurrentConsumption examples to follow the workaround of wake up sequence from standby when using more than one wake up source. Update DAC_SignalsGeneration example to use 2 DACs Channels. Update Flash_Program and Flash_WriteProtection examples to support STM32F091 devices. Add new examples supported only by STM32F091 devices DMA_USARTTransfer USART_8xUsartsOneBoard. ### V1.3.0 / 16-January-2014 Main Changes Update all examples to support the STM32F072 devices and to run on STM32072B-EVAL board. Update all examples folders names to add the peripheral name. Add examples for CAN peripheral. Remove CRC_Example and add three new examples: CRC_32BitsCRCMessage CRC_8BitsCRCMessage CRC_TwoBoards Update TIM_PWMInput example to use SystemCoreClock. ### V1.2.0 / 22-November-2013 Main Changes PWR\PWR_Standby example update to use an accurate LSI clock fre quency. ### V1.1.0 / 31-July-2013 Main Changes Following the changes done in the Template project (EVAL drivers not included in the project source list, 2 workspaces created for STM32F0xx Low-density and Medium-density devices); all readme.txt files were updated to list the additional files to be added in the Template project. IWDG_Reset: decrease the delay to 220 ms All ADC, DAC/DAC_ADC, DMA/ADC_TIM3 and TIM/TIM_ADC_Trigger examples After enabling the ADC, wait until setting of ADC_FLAG_ADRDY flag instead of ADC_FLAG_ADEN COMP\COMP_AnalogWatchdog, FLASH/Write_Protection and RTC/RTC_Timer examples Miscellaneous update ### V1.0.0 / 18-May-2012 Main Changes First official release for STM32F0xx devices ## License Licensed under MCD-ST Liberty SW License Agreement V2, (the "License"); You may not use this package except in compliance with the License. You may obtain a copy of the License at: http://www.st.com/software_license_agreement_liberty_v2 Unless required by applicable law or agreed to in writing, software distributed under the License is distributed on an "AS IS" BASIS, WITHOUT WARRANTIES OR CONDITIONS OF ANY KIND, either express or implied. See the License for the specific language governing permissions and limitations under the License. For complete documentation on STM32 Microcontrollers visit www.st.com/STM32